Stock Lawnmower Derby rules 2024

1. No full wrap around cages. Leg protection bars allowed from front edge of running board to front of rear fender. CAN NOT attach to front or rear bumpers. 1 support from frame to outside of running board on front edge on each side is allowed.
2. No solid tires.
3. Can add/make flat front/rear bumper, NO sharp or pointed bumpers. Uprights on front bumper allowed.
4. Front and rear bumpers can NOT be wider than tires.
5. 25 Hp max engine size. Can swap motors
6. NO frame bracing. Stock frame only.
7. Steering stops and reinforced tie rods allowed.
8. Remove mower decks.